**BOM Button Logic on the LAYOUT Tab of Estimating**   
This much more friendly and more dynamic. Medium paper can be used to make B, C, E or F Flute, etc however, our Raw Materials File only has 1 field for a Shrink Percentage, which can be used as a default. The BOM button you allow you to use the same Medium Materials for all Flutes. So, you can use the same Medium material for each Flute by simply changing the FLUTE Code on the BOM Button. In addition, the Shrink Percentage field that can be modified simply by clicking the Flute Code. Then the program will import the correct Shrink Percentage, which may be adjusted if needed.

For Example, on the estimate below, I have selected C Flute which imports a Shrink Factor of 31.07.   
Our software takes the 40” and divides by (100 – 31.07/100) = 58.029 Inch Medium Length.   
In other words 40” / .6893 = 58.029. A hand calculated formula would be 40” x 1.4507 = 58.028

